Modeling and FDTD Simulation of Dispersive, Gyrotropic, Ferromagnetic Transmission Lines

**Muhammad Shamaas1 and Muhammad Asghar Saqib2**

1, 2Department of Electrical Engineering, University of Engineering and Technology, Lahore 54890, Pakistan

12018msee004@student.uet.edu.pk, 2saqib@uet.edu.pk

**Abstract** –*S*

**Keywords:**I

# Introduction

Ferromagnetic materials are widely used in bulk power transmission and distribution, elecromechanical machines, power electronic converters and radio frequency communication. They have very high magnetic permeability and a strong affinity for magnetic flux so they communicate electromagnetic information using strong magnetic fields. The cyclic magnetization of a Magnetic Material causes many energy losses due to Hysteresis, Eddy currents, Skin effect, Proximity effect, Gyromagnetism, Magnetoresistance, Magnetostriction and other residual losses. It is important to understand their material properties and complex loss mechanisms so that system level models can be developed for their analysis at low and high frequencies.

The three different approaches commonly used for this modeling are calculation, simulation and experimentation. Frequency dependent parasitic core capacitance is responsible for the high frequency self-resonance and frequency limitation of the magnetic core. H. Zhao, Y. Li, Q. Lin, and S. Wang [14] presented a closed form solution for estimating parasitic capacitance of a ferromagnetic core, which stores electric energy in the gradient electric field developed inside the core. The frequency independent power losses due to Ohmic losses were also considered in an equivalent core impedance. The results were verified experimentally and through electromagnetic simulations for the microwave frequency range. N. Shirdel, A. Akbari, H. Mirzaei, and M. Abrishamian [11] presented a FDTD simulation for propagation of UHF Gaussian pulse partial discharges in a dispersive, anisotropic, conductive ferromagnetic transformer core. The model did not include non-linear and gyrotropic nature of the core. J. Xu, M. Koledintseva, Y. Zhang, Y. He, B. Matlin, R. Dubroff, J. Drewniak, and J. Zhang [13] presented an experimental setup for calculating frequency domain behavior of complex permeability and permittivity of a ferromagnetic transmission line. The measured intrinsic impedance and propagation constant was used to determine the per unit length electric transmission line parameters. The results were compared with electromagnetic FDTD simulation and analytical results. The model used genetic algorithm for estimating the transmission line parameters. H. Al-Barqawi, N. Dib and M. Khodier [1] presented a closed form solution for analyzing the electromagnetic fields in a waveguide filled with an anisotropic, dispersive, gyromagnetic ferrite. Two dimensional Finite Difference Time Domain simulation was also carried out for the structure and the frequency variation of propagation constant was studied for the microwave frequency range. The simulation results matched very closely with the analytical closed form solution. The analysis did not account for non-linearity of the magnetic material.

The electric circuit models and laws are not suitable for modeling the behavior of ferromagnetic materials because they are not designed to conduct electric charge upon application of electromotive force. A magnetic circuit must be used for the system level modeling of ferromagnetic materials which transmit magnetic flux as the effective magnetic charge due to the application of Magnetomotive force. The most important magnetic circuit models are the DC Reluctance model, the low frequency Permeance-Capacitance model and the high frequency Magnetic Transmission Line model.

Magnetic Reluctance circuit model [2], based on the G. Ohm’s Law, depicts magnetic core as a Magnetic reluctance which resists the flow of Magnetic Flux. The Reluctance model is only suitable for low frequency steady state simulations of transformers if the reluctance profile of the magnetic core is already known. Better models are needed for modeling the complex behavior of ferromagnetic materials.

R. Buntenbach [2] proposed Power Invariant Permeance-Capacitance Model based on B. Tellegen’s Gyrator Theory. The Permeance-Capacitance model uses a nonlinear permeance to model nonlinearity and hysteresis losses of magnetic materials. The Permeance-Capacitance model is only suitable for low frequency model simulations of ferromagnetic materials. J. Allmeling, W. Hammer, and J. Schonberger [2] presented a permeance-capacitance model for a ferromagnetic transformer core. The circuit adopted a gyrator for the transformation between electric and magnetic domains. Nonlinear permeance elements were used to model core hysteresis losses and magnetic flux leakage. A magnetic conductance was used to represent eddy current losses. Unlike the traditional coupled-inductor model, the transformer magnetic circuit was derived using the core geometry. The model was modified to include Hysteresis, Eddy currents, Piezomagnetism, Magnetoresistance, Magnetostriction and other residual losses. The model did not account for the dispersion characteristics of the magnetic core. M. Luo, D. Dujic, and J. Allmeling [9] presented a permeance-capacitance model for a laminated steel ferromagnetic transformer core to model hysteresis losses and frequency dependent eddy current losses. The non-linear core permeance was designed to approximate the results obtained for a low frequency excitation. The model was not valid for high frequency simulations.

J. Faria [4] – [6] presented Magnetic Transmission Line Model based on the conventional Electric Transmission Line Model. For magnetic transmission lines, transverse impedance and the longitudinal admittance determine the propagation constants for the wave modes. Solutions to Electromagnetic equations were presented in the form of a superposition of natural modes of propagation. Simulations showed that they exhibit super-luminal phase velocity and almost zero attenuation dispersion in the microwave frequency range. The Magnetic Transmission Line exhibited the behavior of a high pass filter.

This research attempts to extend the Magnetic Transmission Line Model for the modeling of dispersive, gyrotropic, ferromagnetic transmission lines, and studying the high frequency response of magnetic transmission line parameters.

# Magnetic Transmission Line Model

The Magnetic Transmission Line Model is useful for modeling linear, dispersive ferromagnetic materials. It provides a closed form solution for electric and magnetic parameters using a system level circuit.

Complex permittivity can be represented as:

The real part is responsible for the displacement current, whereas the imaginary part contributes to the conduction current. During Lorentzian resonance, the lattice vibrations of the atomic harmonic oscillators become extreme, and the electric conductance of the magnetic material increases greatly. Hence the material acts like an electric conductor with a very low resistivity. This resonance causes a peak in electric losses.

Complex permeability can be represented as:

Although Magnetic conduction currents do not exist, Magnetic displacement currents can flow inside a magnetic material. During Lorentzian resonance, the real permeability drops, the magnetic displacement currents are restricted and the magnetic susceptibility falls. This causes failure of the magnetic system.

Analogous to the scalar Electric Potential, scalar magnetic potential can be defined as

The Magnetic Displacement Current is defined as the rate of change of magnetic flux :

The per unit length transverse magnetic inductance represents a magnetic Energy storage element storing magnetic flux:

The per unit length longitudinal capacitance represents an Electric Energy storage element storing electric charge:

The per unit length Magnetic conductance dissipates energy due to Hysteresis, Eddy currents, Skin effect, Proximity effect, Piezomagnetism, Magnetoresistance, Magnetostriction and other residual losses. It is closely related to the magnetic reluctance:

The Magnetic Transmission Line Equations are


The characteristic impedance is the ratio of Magnetic displacement current to the Magnetic Voltage. It is calculated as

# Finite Difference Time Domain Electromagnetic Simulation

MEEP software was used for the electromagnetic simulation of the Gyrotropic, Dispersive, Ferromagnetic Transmission Lines using the Finite Difference Time Domain method which discretizes Maxwell’s Equations using central difference approximations to the space and time partial derivatives. The different field components at a grid location are stored in the edges and faces of a cubic element called Yee’s Cell. The electromagnetic fields are evolved in discrete time steps using leap frog method.

Faraday’s Law can be discretized as follows:

Similarly, Ampere’s Law can be approximated as follows:



MEEP simulator was used to simulate anisotropic, dispersive and gyromagnetic materials.

1. Dispersion Model

Drude-Lorentzian Model models frequency dependent permittivity and permeability. It explains the electrodynamic properties by regarding conduction band electrons as non-interacting electron gas. When the material is excited by an external source of resonant frequency, the material absorption loss increases greatly. Electromagnetic Energy is converted into other forms of energy. Flux Densities contain terms for infinite frequency response and frequency dependent Polarization vector.

and are represented as a sum of harmonic resonances and a term for frequency independent electric conductivity.

is the electrical/magnetic conductivity. is the oscillator strength, is the angular resonance frequency, is a damping factor.

1. Gyrotropy Model

Landau-Lifshitz-Gilbert model describes the precessional motion of saturated magnetic dipoles in a magnetic field.

describes the linear deviation of magnetization from its static equilibrium value. Precession occurs around this unit bias vector . represents oscillator strength, is the angular resonance frequency, is the oscillator damping factor.

# Simulation Results

The

# Discussion

The

# Conclusion

Di

# References

[1] H. Al-Barqawi, N. Dib and M. Khodier, “A Full-Wave Two-Dimensional Finite-Difference Frequency-Domain Analysis of Ferrite-Loaded Structures”. Mosharaka International Conference on Communications, Propagation and Electronics, 2008.

[2] J. Allmeling, W. Hammer, and J. Schonberger, “Transient simulation of magnetic circuits using the permeance-capacitance analogy,” *2012 IEEE 13th Workshop on Control and Modeling for Power Electronics (COMPEL)*, 2012.

[3] S. Blundell, *Magnetism in condensed matter*. Oxford: Oxford University Press, 2014.

[4] J. Faria and M. Pires, “Theory of Magnetic Transmission Lines,” *IEEE Transactions on Microwave Theory and Techniques*, vol. 60, no. 10, pp. 2941–2949, 2012.

[5] J. Faria, “Formulation of Multiwire Magnetic Transmission-Line Theory”, *Progress in Electromagnetics Research B*, Vol. 49, 2013.

[6] J. Faria, “A physical model of the ideal transformer based on magnetic transmission line theory”, *Journal of Electromagnetic Waves and Applications*, Vol. 27, No. 3, 2013.

[7] “IEEE Standard for Pulse Transformers," in ANSI/IEEE Std 390-1987, vol., no., pp.1-32, 14 Oct. 1987.

[8] “IEEE Recommended Practice for Validation of Computational Electromagnetics Computer Modeling and Simulations," in IEEE Std 1597.2-2010, vol., no., pp.1-124, 25 Feb. 2011.

[9] M. Luo, D. Dujic, and J. Allmeling, “Permeance based modeling of magnetic hysteresis with inclusion of eddy current effect,” *2018 IEEE Applied Power Electronics Conference and Exposition (APEC)*, 2018.

[10] A. Oskooi, D. Roundy, M. Ibanescu, P. Bermel, J. Joannopoulos, and S. Johnson, “MEEP: A flexible free-software package for electromagnetic simulations by the FDTD method”, *Computer Physics Communications*, Vol. 181, pp. 687-702, 2010.

[11] N. Shirdel, A. Akbari, H. Mirzaei, and M. Abrishamian, “Three-dimensional simulation of UHF signal propagation in transformer using FDTD method,” *2011 International Conference on Power Engineering, Energy and Electrical Drives*, 2011.

[12] A. Taflove and S. Hagness, *Computational Electrodynamics: The Finite-Difference Time-Domain Method*, 3rd ed. Boston: Artech House, 2005.

[13] J. Xu, M. Koledintseva, Y. Zhang, Y. He, B. Matlin, R. Dubroff, J. Drewniak, and J. Zhang, “Complex Permittivity and Permeability Measurements and Finite-Difference Time-Domain Simulation of Ferrite Materials,” *IEEE Transactions on Electromagnetic Compatibility*, vol. 52, no. 4, 2010.

[14] H. Zhao, Y. Li, Q. Lin, and S. Wang, “The Parasitic Capacitance of Magnetic Components with Ferrite Cores Due to Time-Varying Electromagnetic (EM) Field,” *2018 IEEE Energy Conversion Congress and Exposition (ECCE)*, 2018.